IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0]"
Description: "Option [BaseQuantities:Off]"
Description: "Option [GridExport:On]"
Description: "Option [Assemblies:On]"
Description: "Option [Bolts:On]"
Description: "Option [Rebars:On]"
Description: "Option [PourObjects:Off]"
Description: "Option [Welds:On]"
Description: "Option [SurfaceTreatments:On]"
Description: "Option [LocationBy:0]"
Description: "Option [ViewColors:Off]"
Description: "Option [SectionedSpine:Off]"
Description: "Option [PropertySets:On]"
Description: "Option [Export all:Off]"
File name: "EO37- --1.ifc"
Time stamp: "2020-02-28T15:05:44"
Author: "SWECO\FILANG"
Organization: "Structural Designer"
Preprocessor: "IFC Database Version: Work"
Originating system: "Tekla Structures 2017i Service Pack 7, IFC Export Version: 4.0.0.0 Feb 8 2019"
Application: "Tekla Structures" version "2017i Service Pack 7" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation"

People and organizations
  Person "Undefined" id "SWECO\FILANG" of Organization "Trimble Solutions Corporation"
  Owner history of Person "Undefined" id "SWECO\FILANG" of Organization "Trimble Solutions Corporation" | application "Tekla Structures" version "2017i Service Pack 7" identifier "Multi material modeling" by Organization "Trimble Solutions Corporation" | change NOCHANGE | created 1582895144 (2020-02-28T13:05:44Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Undefined"
  IFCSITE "Undefined" | elevation above sea level 0.
    IFCBUILDING "Lohko 1"
      IFCBUILDINGSTOREY "1. kerros" | elevation 0.
        contains 1 element
          1 x IFCELEMENTASSEMBLY | REINFORCEMENT_UNIT | names: "ONTELOLAATTA" | parts: 2 IFCBEAM | property sets: BEC, BEC-Työnkulku, Tekla Assembly

Property sets
  BEC | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Betoniosien tilavuus = 1.3509 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Elementin Pieli pinta-ala = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Elementin aukkojen pinta-ala = 0.05527 (IFCAREAMEASURE) [SQUARE_METRE]
    Elementin betoniosien korkeus = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    Elementin betoniosien paksuus = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Elementin betoniosien pituus = 5753.60581 (IFCLENGTHMEASURE) [MILLI METRE]
    Elementin brutto pinta-ala = 6.90433 (IFCAREAMEASURE) [SQUARE_METRE]
    Elementin juokseva numero, ACN (no value)
    Elementin kerros = "1. kerros" (IFCLABEL)
    Elementin lohko = "Lohko 1" (IFCLABEL)
    Elementin netto pinta-ala = 6.84906 (IFCAREAMEASURE) [SQUARE_METRE]
    Elementin nimi = "ONTELOLAATTA" (IFCLABEL)
    Elementin numerointisarja = "EO37- -" (IFCLABEL)
    Elementin paino = 3393.92089 (IFCMASSMEASURE) [KILO GRAM]
    Elementin piirustusnumero = "EO37- --1" (IFCLABEL)
    Elementin pääosan materiaalin tyyppi = "CONCRETE" (IFCLABEL)
    Elementin pääosan profiili = "EO37" (IFCLABEL)
    Elementin raudoituksen paino = 0. (IFCMASSMEASURE) [KILO GRAM]
    Elementin raudoitusarvio (no value)
    Elementin tyyppi = "Precast" (IFCLABEL)
    Elementti Aukkojen lkm = 1 (IFCINTEGER)
    Elementtitehtaan status (no value)
    Elementtitunnus = "EO37- --1" (IFCLABEL)
    GUID = "72D37E98-6E9E-429E-A96C-9BDE40F7F381" (IFCLABEL)
    Kokoonpano hierarkiataso = 0 (IFCINTEGER)
    O_KL_Aukot jm = 1164.95018 (IFCLENGTHMEASURE) [MILLI METRE]
    O_KL_Bruttoala = 6.90433 (IFCAREAMEASURE) [SQUARE_METRE]
    O_KL_Bruttoala = 6.90433 (IFCAREAMEASURE) [SQUARE_METRE]
    O_KL_Eriste = "" (IFCLABEL)
    O_KL_Eristeen_paksuus = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    O_KL_Laatan kavennus jm = 11027.20605 (IFCLENGTHMEASURE) [MILLI METRE]
    O_KL_Nettoala = 6.70926 (IFCAREAMEASURE) [SQUARE_METRE]
    O_KL_Syvennykset jm = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    O_KL_Tunnus = "" (IFCLABEL)
    O_KL_Vinopään sahaus kpl = 0 (IFCINTEGER)
    Palkkielementin uuman leveys = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Palkkielementti, leuka 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Palkkielementti, leuka 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Seinäelementti, eristeen materiaali = "" (IFCLABEL)
    Seinäelementti, eristeen paksuus = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Seinäelementti, pintakäsittely 1 = "" (IFCLABEL)
    Seinäelementti, pintakäsittely 2 = "" (IFCLABEL)
    Seinäelementti, pintakäsittely 3 = "" (IFCLABEL)
    Seinäelementti, pintakäsittelyala 1 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Seinäelementti, pintakäsittelyala 2 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Seinäelementti, pintakäsittelyala 3 = 0. (IFCAREAMEASURE) [SQUARE_METRE]
    Seinäelementti, sisäkuoren materiaali = "" (IFCLABEL)
    Seinäelementti, sisäkuoren paksuus = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Seinäelementti, sisäkuoren tilavuus = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Seinäelementti, ulkokuoren materiaali = "" (IFCLABEL)
    Seinäelementti, ulkokuoren paksuus = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Seinäelementti, ulkokuoren tilavuus = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Sijainti modulilinjoilla = "3-4/D-F" (IFCLABEL)
    TT-Laatan ripaleveys = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Teräskokoonpano Nimi = "ONTELOLAATTA" (IFCLABEL)
    Teräskokoonpano bruttopaino = 3425.60091 (IFCMASSMEASURE) [KILO GRAM]
    Teräskokoonpano nettopaino = 3393.92089 (IFCMASSMEASURE) [KILO GRAM]
    Teräskokoonpano tunnus = "EO37- --1" (IFCLABEL)
    Valutarvikkeen Elementtitunnus (no value)
    Valutarvikkeen class = "243" (IFCLABEL)
    Valutarvikkeen tuotetieto (no value)
  BEC-Työnkulku | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    10 RAK-suunnittelu, status (no value)
    11 RAK-suunnittelu, status, pvm (no value)
    12 RAK-suunnittelu, kommentti (no value)
    20 ELE-suunnittelu, status (no value)
    21 ELE-suunnittelu, status, pvm (no value)
    22 ELE-suunnittelu, kommentti (no value)
    23 ELE-piirustus, nimi = "C [EO37- -.1 - 1]" (IFCLABEL)
    24 ELE-piirustus, pvm (no value)
    25 ELE-piirustus, muutos = "" (IFCLABEL)
    26 ELE-piirustus, muutos, pvm = 0 (IFCTIMESTAMP)
    27 ELE-suunnitelma tarvitaan, pvm (no value)
    28 ELE-suunnitelma valmis, pvm (no value)
    30 Valmistus, betoni, status (no value)
    31 Valmistus, betoni, status, pvm (no value)
    32 Valmistus, teräs, status (no value)
    33 Valmistus, teräs, status, pvm (no value)
    34 Valmistus, kommentti (no value)
    35 Valmistus, tehdas (no value)
    36 Valmistus, ID (no value)
    37 Valmistus, suunniteltu valu, pvm (no value)
    38 Valmistus, toteutunut valu, pvm (no value)
    39 Valm. sis. suunn., status (no value)
    39b Punostieto (no value)
    40 Toimitus, suunniteltu, pvm (no value)
    41 Toimitus, toteutunut, pvm (no value)
    42 Kuormanumero (no value)
    43 Kuormakirja (no value)
    44 Toimitus kommentti (no value)
    50 Asennus, status (no value)
    51 Asennus, kommentti (no value)
    52 Asennus, suunniteltu, pvm (no value)
    53 Asennus, toteutunut, pvm (no value)
    54 Asennus, jälkivalu, pvm (no value)
    55 Asennusjärjestys (no value)
  Tekla Assembly | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Assembly/Cast unit Mark = "EO37- --1" (IFCLABEL)
    Assembly/Cast unit bottom elevation = "-0.586" (IFCLABEL)
    Assembly/Cast unit position code = "3-4/D-F" (IFCLABEL)
    Assembly/Cast unit top elevation = "+0.138" (IFCLABEL)
    Assembly/Cast unit weight = 3393.9 (IFCMASSMEASURE) [KILO GRAM]
    Cast unit rebar weight = 0. (IFCMASSMEASURE) [KILO GRAM]
    Control number (no value)
  Tekla Common | properties | on 1 object (1 IFCBEAM)
    Bottom elevation = "-0.586" (IFCLABEL)
    Class = "243" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "-0.236" (IFCLABEL)
  Tekla Common | properties | on 1 object (1 IFCBEAM)
    Bottom elevation = "-0.421" (IFCLABEL)
    Class = "243" (IFCLABEL)
    Initial GUID (no value)
    Phase = 1 (IFCINTEGER)
    Preliminary mark = "" (IFCLABEL)
    Top elevation = "+0.138" (IFCLABEL)
  Tekla Quantity | properties | on 1 object (1 IFCBEAM)
    Area per tons = 923.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 6.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 5493.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 15.4 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 16.7 (IFCMASSMEASURE) [KILO GRAM]
    Width = 170. (IFCLENGTHMEASURE) [MILLI METRE]
  Tekla Quantity | properties | on 1 object (1 IFCBEAM)
    Area per tons = 11.5 (IFCAREAMEASURE) [SQUARE_METRE]
    Gross footprint area = 6.9 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 370. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 5753.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Net surface area = 38.8 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Weight = 3377.3 (IFCMASSMEASURE) [KILO GRAM]
    Width = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ER-1" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete_EO37- --1-1" (IFCIDENTIFIER)